                              Custom elevation data file: 
                                Show topographic overlay: False
                               Show low altitude overlay: False
                                 Show hill slope overlay: False
                               Show projected video feed: False
                                Low altitude warning (m): 9.1440000
                         Airspace indicator altitude (m): 120.0000000
                        Rangefinder obstacle warning (m): 30.0000000
                                     Vector overlay file: 
                                     Raster overlay file: 
                             Waypoint snap altitude mode: Above Ground Level
           Waypoint snap altitude above ground level (m): 15.2400000
       Waypoint snap altitude above takeoff location (m): 20.0000000
                     Waypoint mission cruise Speed (m/s): 10.0000000
                                Waypoint curve range (m): 0.9144000
                  Vertical flight path to first waypoint: Safe
                       Max number of waypoints to upload: 1000
                                          Transect Usage: Just Flying
                      Transect Zig-Zag Heading (degrees): -25.1031826
                               Transect Spacing (meters): 15.2400000
                    Transect Overshoot Distance (meters): 0.0000000
                                Most recent payload type: None
             Most recent flight controller firmware type: Px4
                       Most recent rangefinder equipment: None
                                             Basemap URL: https://gis.apfo.usda.gov/arcgis/rest/services/NAIP/USDA_CONUS_PRIME/ImageServer/tile/{z}/{y}/{x}?blankTile=false
                               Basemap extra HTTP header: 
                                         Basemap save as: png
                                       Basemap subfolder: naip
                                       Basemap copyright: U. S. Department of Agriculture, Farm Service Agency
                                        Basemap max zoom: 17
                                        Basemap min zoom: 0
                               Basemap min zoom fallback: OpenStreetMap Carto
                                      Custom basemap URL: 
                        Custom basemap extra HTTP header: 
                                  Custom basemap save as: png
                                Custom basemap subfolder: 
                                 Custom basemap max zoom: 17
                                 Custom basemap min zoom: 0
                        Custom basemap min zoom fallback: OpenStreetMap Carto
                                    Copernicus config Id: 
                                           App System Id: 218
                                        App Component Id: 0
                                        Drone connection: IP
                               Drone IP address and port: 192.168.144.20:0
                        Drone IP address is WiFi gateway: False
                                Drone transport protocol: UDP
                             Drone connection local port: 14550
                                 Drone network interface: eth0
                                 Custom drone connection: N/A
             Custom drone connection IP address and port: 
        Custom drone connection is to IP of WiFi gateway: False
              Custom drone connection transport protocol: UDP
                      Custom drone connection local port: 0
                          Custom drone network interface: 
                                   Video stream protocol: RTSP
              DA video server IP address is WiFi gateway: False
       Second stream DA video server IP address and port: 
                                                RTSP URL: rtsp://192.168.144.20:8553/stream2
                                  Second stream RTSP URL: 
                                 Video network interface: eth0
                            Custom Video stream protocol: N/A
       Custom DA video server IP address is WiFi gateway: False
Custom second stream DA video server IP address and port: 
                           Custom second stream RTSP URL: 
                          Custom video network interface: 
                                         Relay mode port: 0
                                 Relay network interface: 
                           Relay mode disable encryption: False
                                             Drone color: Red
                                                   Units: Imperial (mph)
                                          Lat/Lng format: Decimal Degrees
                            Show Horizontal Ground Speed: True
                                     Show Vertical Speed: True
                                            Show Lat/Lng: False
                                 Show Distance from Home: True
                         Show Alt MSL from Elevation Map: False
            Show Alt MSL from inputted takeoff elevation: False
                          Inputted takeoff elevation (m): 0.0000000
          ADSB audible warning cylinder altitude (m MSL): 3000.0000000
                ADSB audible warning cylinder radius (m): 6000.0000000
                                         Always show HUD: False
                      Always show camera control sidebar: False
                                            Hide minimap: False
                                    Show battery voltage: False
                                Minimap/Minivideo corner: Bottom Right
                                          Developer mode: False
                    Flight log entry display time format: Flight Time
                              Simulator takeoff latitude: 42.9389020
                             Simulator takeoff longitude: -122.1459840
                                       Simulated payload: None
                                         Simulate Strobe: False
                                   Simulate Rangefinders: False
                                   Log simulated flights: False
                  Dont connect this app to the simulator: False
                                  Ignis drop spacing (m): 10.0000000
                               Ignis max drop period (s): 7.0000000
                            Ignis ground drop timing (s): 0.0000000
                 Ignis drop location persistence (hours): 24.0000000
                                      DART fuse time (s): 90.0000000
                 Mosquito dropper number of cones loaded: 23
                        Photo Interval (s, 0 for Single): 0.0000000
        Wiris thermal horizontal field of view (degrees): 32.0000000
                                        Bindings profile: Custom
                            Pitch/yaw/zoom sticks scalar: 1.0000000
                                            Pitch gimbal: Unbound
                                              Yaw gimbal: Unbound
                                             Zoom camera: Unbound
                                         Recenter gimbal: Unbound
                         Go to secondary gimbal position: Unbound
                                 Recenter position pitch: 0.0000000
                                  Secondary position yaw: -180.0000000
                                Secondary position pitch: 0.0000000
                            Toggle pitch/yaw or recenter: Unbound
                           Toggle pitch/zoom or recenter: Unbound
                          Increase exposure compensation: Unbound
                          Decrease exposure compensation: Unbound
                       Switch video feed / record (hold): Unbound
               Shoot single photo / start interval photo: Unbound
                                     Stop interval photo: Unbound
                                   Start recording video: Unbound
                                    Stop recording video: Unbound
                                   Minimize/maximize map: Unbound
                                       Enable chase mode: Unbound
                                        Mark rangefinder: Unbound
                                        Drop one payload: Unbound
                                Enable Corning Shark 410: False
                                  FPV Camera orientation: 0.0000000
                                   Enable RTK Forwarding: False
                                 Set Offboard Flightmode: Unbound
